**(do not use if tenders referencing 2020 SSBC)**

**Amendment to Section 10, Heavy Rock Riprap, of the 2017 Standard Specifications for Bridge Construction, Re: Class 1M Material Dimensions**

The nominal diameter for Class 1M heavy rock riprap, for the 20% to 50% shown in Table 10-1 of Subsection 10.3, **Heavy Rock Riprap Material**, is revised from 1 200 mm to *200 mm*.