**Amendments to Specification 3.31, asphalt pavement crack sealing**

1. Subsection 3.31.5.1, **Acceptance Sampling and Testing of Crack Sealant,** replace the last paragraph in its entirety with the following:

The Department will determine the frequency of testing of sealant. Cold pour materials that do not conform to the Specification limits shall result in a unit price adjustment for each metre of crack in the Lot in accordance with Table 3.31.6.

1. Subsection 3.31.6, **MEASUREMENT AND PAYMENT,** is replaced in its entirety with the following:

Measurement will be made in metres of the length of the cracks on which crack sealing has been performed.

Payment will be made at the unit price bid per metre for "Crack Sealing" subject to the unit

price adjustments specified herein. This payment will be full compensation for cleaning the road surface adjacent to the cracks, supplying and applying the crack sealant, blotting agent, quality control, traffic accommodation and signing.

The following unit price adjustments apply only to EC-101 or other approved cold pour materials and do not relieve the Contractor of the requirements to complete the Work in accordance with these specifications.

**TABLE 3.31.6**

**LOT UNIT PRICE ADJUSTMENTS**

|  |  |
| --- | --- |
| **Requirement** | **Unit Price Adjustment** |
| Solids (%)  ≥ 59  58.9 to 54.0  53.0 to 49.0  < 49 | No Adjustment  5%  10%  15% |

The unit price applicable to each Lot quantity of "Crack Sealing" shall be as follows:

Lk = BP - (BP \* AF)

Where: Lk is the Lot Unit Price per metre;

BP is the Contract Bid Price per metre; and

AF is the Adjustment Factor for the Crack Sealant.