**Amendment to Specification 3.33, Crack Repair – Spray Patch**

Subsection 3.33.4, PROCEDURE**,** is revised as follows:

1. Delete the second sentence in the first paragraph, reading “Generally, cracks with a width of less than 5 mm will not require repair.”

Subsection 3.33.5, SCHEDULE LIMITATION**,** is revised as follows:

1. Delete the words, “minimum of two weeks” and replace with “minimum of 7 days”.