Farm: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date Plan Created: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Emergency Telephone Numbers: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Farm Owner/Main Contact: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Alternate Contact: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

NRCB 24-hour Response Line: **1-866-383-6722** Emergency: **911**

County Bylaw Officers: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Other Contacts: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |
| --- |
| **Manure Spill in Farm Yard or Breach of Manure Storage** |
| Your Plan: |
| General action steps: Stop flow into storage, notify NRCB and other authorities if impacting a water body or water source (such as a well or dugout), build containment dams, add soil to berm, pump manure from storage to field or alternative storage (such as a tank or other manure storage facility), remove and clean up manure from discharge area. Prepare summary report. |
| **Manure Spill on Road** |
| Your Plan: |
| General action steps: Assess the situation. Human injuries, if present, take precedence. Prevent further accidents or injuries by putting out warning signs such as flashers, flares or triangles. Stop any oncoming traffic, stop any additional spillage, try to contain the manure released or spilled, and remove any that can be done without disruption to the road. Contact county bylaw officer, the county sheriff or RCMP and the NRCB. Remove any remaining manure from road under advisement. Prepare summary report. |
| **Manure Dragline or Pumping Emergency** |
| Your Plan: |
| General action steps: Stop pumps, close valves, separate or clamp pipes, build containment dams, notify the landowner and the NRCB, remove and clean up manure from discharge area. Prepare summary report. |
| **Manure Spill in Field** |
| Your Plan: |
| General action steps: Stop manure application, build containment dams, plow a diversion trench, remove and clean up manure from discharge area, notify the landowner and NRCB. Prepare summary report. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Additional Equipment, Contractors and Storage** | **Location** | **Owner** | **Telephone No.** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |
| --- |
| **Summary Report** |
|  |