**Amendment to Specification 5.5, Supply of Portland Cement Concrete**

Subsection 5.5.2.1 **Portland Cement,** is revised as follows:

1. Add the following sentences to the second paragraph,

“Portland Limestone Cement (GUL) may be used in the construction of items identified in Specification 4.2 Concrete Curbs, Gutters, Sidewalks, Medians and Traffic Islands. Portland Limestone Cement shall conform to the requirements of Specification 5.11, Supply of Portland Cement, and concrete products in accordance with CSA A23.1.”